ALYNE

The Alyne is made with slim and compact vertical flat columns which stylishly curve at the top.

Product: Electric horizontal radiator

Pre-installed: Prefilled with oil, equipped with a thermostat and a 1,2 m insulated cable with plug.

Also supplied: Brackets, screws, plugs and manual

Control: Control via an integrated thermostat with automatic weekly programming, open window detection, presence detection and boost function.

Packaging: Every radiator is sturdily packaged in high-quality cardboard. The radiator’s characteristics are shown on the label: electric power – height – length.

Warranty: 10 years for the radiator and 2 years for the electrical components, as long as the installation instructions have been followed, Stelrad’s warranty conditions have been met and the radiator is installed outside the splash area.

Paint process: All radiators are degreased, phosphated, primed and powder-coated.

Colour: Traffic white

Conformity: EcoDesign 2018 (EU Regulation 2015/1188)

Technical data: Voltage 230V ~50Hz, IP24, Class II

Height: 580 mm

Lengths: 580 | 820 | 980 mm

Depth: 90 mm

Output: 1.000 | 1.500 | 1.800 W