COLUMN

The Column is the retro radiator with contemporary thermal comfort. The beautiful design comes into its own in both classic and modern interiors. The radiator is available in a horizontal and vertical version.

Product: column radiator with 4 connections

Also supplied: Brackets with anti-lift, 4 pieces up to length 854 mm and 6 pieces from length 1.038 mm, screws, plugs, air vent, blind plug and installation instructions

Connections: 4 x ½” female side connection.

Packaging: Every radiator is sturdily wrapped in plastic. The radiator’s characteristics are shown on the label: type – height – length.

Warranty: 10 years, as long as the installation instructions have been followed and Stelrad’s warranty conditions have been met.

Paint process: All radiators are degreased, phosphated and powder-coated in Stelrad white 9016 as standard.

Colours: Stelrad white 9016 + 35 different Stelrad colours and about 200 RAL-colours are possible

Max. operating pressure: 10 bar (tested to 13 bar)

Max. operating temperature: 110 °C

Conformity: in accordance with EN442

Quality assurance: NF

Number of columns: 2 | 3 | 4

Heights: 300 | 500 | 600 | 750 and 1.800 | 2.000 | 2.500 mm

Lengths: 440 – 1.866 mm and 348 | 440 mm

Depths: 66 | 107 | 148 mm