PLANAR 8

The Planar 8 is with a flat front, perfectly fitting side panels and upper grille a decorative radiator with a timeless design. Furthermore you have, thanks to the 4 side- and 4 bottom connections, a variety of connection possibilities. This makes the Planar 8 easy to install and applicable in about every situation. In addition, it offers a uniform wall distance of 65 mm for all types at the center connection.

Product: decorative valve radiator with a flat front and 8 connections

Finishing: decorative flat front, upper grille and side panels

Pre-installed: preset valve insert, air vent and blind plugs

Valve insert: The integrated adjustable valve insert (without thermostatic head) is factory-fit on the right side of the radiator, tested in accordance with EN215 and compatible with thermostatic heads M30 x 1,5 mm.

The thermostatic valve insert is factory-set in relation to the size of the radiator. This presetting ensures optimum throughput in the radiator. Factory setting for two-pipe systems, also suitable for one-pipe systems (as long as the valve insert is adjusted to position 8).

Also supplied: Monclac brackets with anti-lift (VDI compliant when used in combination with included anti-slide clips), screws, plugs and installation instructions

Connections: 4 x ¾” male Eurocone bottom connection (2 x centre and 2 x lateral)and 4 x ½” female side connection. Uniform wall distance of 65 mm for all types at the center connection. Left-hand version of types 21-33 available on request. This changes the distances between the connections and the wall for types 22 and 33.

Lugs: Type 11 is equipped with 2 pairs of mounting lugs up to 1.600 mm and 3 pairs from
1.800 mm

Packaging: Every radiator is sturdily packaged in high-quality cardboard and wrapped in plastic. The radiator’s characteristics are shown on the label: type – height – length.

Warranty: 10 years, as long as the installation instructions have been followed and Stelrad’s warranty conditions have been met.

Paint process: All radiators are degreased, phosphated, cataphoretically primed and powder-coated in Stelrad white 9016 as standard.

Colours: Stelrad white 9016 + 35 different Stelrad colours and about 200 RAL-colours are possible

Max. operating pressure: 10 bar (tested to 13 bar)

Max. operating temperature: 110 °C

Conformity: in accordance with EN442

Quality assurance: NF

Types: 11 | 21 | 22 | 33

Heights: 300 | 400 | 500 | 600 | 700 | 900 mm

Lengths: 400 – 3.000 mm

Depths: 63 | 79 | 102 | 160 mm